<http://students.iitk.ac.in/eclub/assets/tutorials/USBKeyboard.pdf>

some imporant point for running code properly

we need to download usb hostshield rev 2.0 version library from [www.github.com](http://www.github.com)

for various header files included in code for using special functions.one more important thing which we need to do after downloading the library is to uncomment a #define code written inside avrpin library's H file.

This uncommenting is required only if we are using Arduino Mega ADK board with MAX3421e built-in.